1. Highlights
2. Volume and biomass concentration are the more relevant variables for loss minimization
3. The batch reactor was successfully simulated using PINN
4. PINNs were not capable of appropriately simulate reactors with volume variation
5. Strategies for simulating reactors with volume in transient state are suggested